Hi Kartik,

We need to implement the quiz for Safety Equipment page, same way as applied to Fatality Breakdown, giving points to user only if they reaches the 75% of certainty.

Please see below the questions and answer (right answer highlighted) for each section:

For Construction/ Hard Hat:

**Questions:**

1. True or False: Wearing Hard Hats is optional on a construction site:
   1. True
   2. False
2. How many Types of Head protection is there?
   1. 1 Type
   2. 3 Types
   3. 2 Types
   4. 5 Types
3. Which class of protective headwear must be used when working with non-conducting material?
   1. Class C
   2. Class E
   3. Class G
   4. Class E and G
   5. All of the above
4. True or False: It is important that the hard hat is CSA certified and is properly fitted to a workers head.
   1. True
   2. False

For Construction/ Safety Boots:

**Questions:**

1. True or False: Foot protection is only required on construction sites?
   1. True
   2. False
2. When selecting foot protection workers should ensure that they:
   1. Fit snugly around the heel and ankle
   2. Has plenty of toe room
   3. Is comfortable
   4. All of the above
3. What section of Regulation 213/91 for Construction Projects talks about protective footwear use:
   1. O. Reg 213/91 s. 21
   2. O. Reg 213/91 s. 22
   3. O. Reg 213/91 s. 23
   4. There is no section that discusses footwear.
4. CSA approved protective footwear is required to have several labels attached to it, what are some of these labels?
   1. Green triangle
   2. White rectangle with a tree symbol
   3. White rectangle with a yellow symbol
   4. Both A and B

For Construction/ Eye Protection:

**Questions:**

1. True or False: Safety glasses are optional, if workers do not want to wear them they don’t have to.
   1. True
   2. False
2. How many Classes of safety glasses are identified in the CSA Standard?
   1. 3
   2. 7
   3. 5
   4. There are no classes
3. How often should safety glasses be inspected and cleaned?
   1. Once in a while
   2. Once a week
   3. Daily
   4. Never
4. If an inspection shows the safety glasses are scratched employees should:
   1. Throw them away immediately
   2. Wear them for the day and then get new ones
   3. Refuse to work
   4. Continue to wear them until they break and then replace them.

For Construction/Fall Protection Harness:

**Questions:**

1. True or False: Fall protection is only one component of a fall protection system.
   1. True
   2. False
2. How many classes of full body harnesses are there?
   1. 3
   2. 5
   3. 7
   4. 4
3. What class of full body harness aids in the position of a worker?
   1. Class L
   2. Class A
   3. Class P
   4. Class B
4. What section of O. Reg. 213/91 relates to fall protection?
   1. Section 26
   2. Section 22
   3. Section 36
   4. Section 30

For Construction/ Safety Gloves:

**Questions:**

* 1. True or False: Gloves are only required for workers using chemicals that may harm or burn their skin.
     1. True
     2. False
  2. What are some of the groups of gloves available to protect workers skin?
     1. Leather
     2. Coated fabric
     3. Mesh
     4. All of the above
  3. What section of O. Reg. 213/91 for Construction Projects enforces the use of skin protection?
     1. Section 22
     2. Section 25
     3. Section 29
     4. Section 21
  4. What are some things workers should consider before selecting their safety gloves?
     1. Length of exposure
     2. Temperature
     3. Color
     4. Both A and B

Regards,